microSD Duplicator - microSD200PC

Nexcopy introduces the all new microSD duplicator flash card copier, the microSD200PC.  The microSD Duplicator is specifically designed for the microSD form factor and does not require SD adapter cards.

With the microSD duplicator being specifically designed for the microSD flash media, production time increase by over 30% because the user is no longer swapping microSD media out of SD card adapters.  This system provides the most stable and reliable platform for small media or microSD duplication.  The microSD Duplicator is available in 20, 40 and 60 target systems.

With user friendly software interface and powerful copy features, you can copy to 20 blank microSD flash memory cards, simply and automatically. No “copy-n-paste.” No adapter card loading. No hassles. The unit is a PC Based microSD Duplicator capable of copying at maximum data transfer speeds.

microSD Duplicator Key Features

    » Copy 20 microSD cards automatically
    » Support SDHC media class
    » SD adapter cards are NOT required
    » User friendly software interface with Job Wizard
    » Low Level bit-for-bit Copy option
    » Volume naming option for flash memory ID
    » Format feature for those pesky unformatted cards
    » Full verification function to ensure accuracy
    » Contemporary design with heavy duty case for 24/7 operation
    » Supports FAT, FAT32 & NTFS*
    » No Enumeration time for microSD media

Learn more about the microSD200PC microSD Duplicator system.  The microSD Duplicator is also available in 40 and 60 target systems.

microSD200PC Specifications

    » Operating Environment: PC Based
    » Copies all Audio / Video / Data
    » Power: Auto detects 120 / 240
    » Weight 6.8 lbs / 3.08 kg
    » Dimensions LxWxH (mm) 220 x 200 x 130

PC System Requirements

    » 1.8GHz Dual Core Processor or 2.0GHz Processor or better
    » 1GB RAM or 2GB for optimal performance
    » Windows XP SP2
    » 2 USB 2.0 high speed port
    » Windows .NET Frameworks (Provided)
    » Disconnect Network & Mapped drives


*Product specifications can change without notice. Monitor not included.
*NTFS support in bit-for-bit copy mode only.