<p>
Nexcopy duplicators:  Advanced copy functions. Small foot print. Simple to operate.
</p>
<p>
Economical solutions for data loading and data distribution via flash memory.
</p>
<p>
Easy as a photocopier.  Capable of copying at your flash drives maximum transfer speed.
</p>

<ul>
<li>8 and 16 socket systems available, no PC required</li>
<li>Binary copier, supports bootable devices</li>
<li>Any format supported, FAT, FAT32, NTFS, Ext4, HFS, etc</li>
<li>Up to 1,800MB/s transfer speed to each port</li>
<li>Asynchronous duplication for masters up to 256MBs</li>
<li>Copy, Copy + Verify, Compare, Erase, QC testing and more</li>
<li>Powerful 32-bit CRC data error checking</li>
<li>DoD (Department of Defense) erase function</li>
<li>USB benchmark speed tests</li>
<li>Memory H2 integrity testing</li>
<li>USB information and capacity check</li>
<li>Real Time performance feedback via LCD</li>
<li>Auto start once unit is fully populated</li>
<li>Contemporary design with heavy duty case for 24/7 operation</li>
</ul>

<ul>
<li>MODELS</li>
<li>CF107SA</li>
<li>CF115SA</li>
</ul>

<p>CF107SA SPECIFICATIONS</p>

<ul>
<li>Copies to 7 flash devices</li>
<li>Buffer Memory of 256MBs</li>
<li>LCD Display 2x20 Characters, Backlit</li>
<li>Operating Environment: Standalone</li>
<li>Copies all Audio / Video / Data</li>
<li>Binary copier</li>
<li>Copy boot code and partition tables</li>
<li>Power: Manual switching for 120 / 230</li>
<li>Weight 6.2 lbs / 2.8 kg</li>
<li>Operating Temp: 41F ~ 122F</li>
<li>Operating Humidity: 15% ~ 85%</li>
<li>Dimensions LxWxH (mm) 317 x 184 x 184</li>
</ul>

<p>CF115SA SPECIFICATIONS</p>

<ul>
<li>Copies to 15 flash devices</li>
<li>Buffer Memory of 256MBs</li>
<li>LCD Display 2x20 Characters, Backlit</li>
<li>Operating Environment: Standalone</li>
<li>Copies all Audio / Video / Data</li>
<li>Binary copier</li>
<li>Copy boot code and partition tables</li>
<li>Power: Manual switching for 120 / 230</li>
<li>Weight 11.3 lbs / 5.2 kg</li>
<li>Operating Temp: 41F ~ 122F</li>
<li>Operating Humidity: 15% ~ 85%</li>
<li>Dimensions LxWxH (mm) 3521 x 184 x 250</li>
</ul>

<p>Product specifiations can change without notice.  Contact Nexcopy for details.  Nexcopy is not responsible for errors posted as either text or images on reseller websites.</p>