<p>
Nexcopy duplicators:  Advanced copy functions. Small foot print. Simple to operate.
</p>
<p>
Economical solutions for data loading and data distribution via flash memory.
</p>
<p>
Easy as a photocopier.  Capable of copying at your flash drives maximum transfer speed.
</p>

<ul>
<li>Create USB Read Only Partitions
<li>Create USB CDROM partitions
<li>Write Protect 1st partition, 2nd partition or both
<li>Make USB Read Only so data cannot be deleted
<li>Control hard coded USB serial numbers
<li>Serial number includes 10 character prefix option
<li>Sequential serial number control
<li>Create USB specific IMG files
<li>Write Protect bootable USB partitions
<li>Nexcopy certified USB media is required
<li>Partition 20 USB flash drives automatically
<li>High Speed USB 2.0
<li>User friendly software interface
<li>Reset USB device without partitions
<li>Volume naming option for flash drive ID
</ul>

<ul>
<li>MODELS</li>
<li>USB160PRO</li>
<li>USB200PRO</li>
</ul>

<P>ADVANCED FEATURES</P>

<ul>
<li>Create USB partitions</li>
<li>Create CD-ROM partitions *ISO file size limitation</li>
<li>Write Protect first partition, second partition or both</li>
<li>Make USB Read only so data cannot be deleted</li>
<li>Control hard coded serial numbers on USB</li>
<li>Serial number includes optional 10 character prefix control</li>
<li>Create USB specific IMG files for bootable drives</li>
<li>Write protect bootable partitions</li>
</ul>

<p>USB160PRO SPECIFICATIONS</p>

<ul>
<li>Host PC requirements:</li>
<li>2.0 Dual Core Processor or better</li>
<li>2GB RAM</li>
<li>Windows XP (SP 2+) or Windows 7 32/64</li>
<li>One USB 3.0 High Speed Port</li>
<li>Windows .NET Installed</li>
<li>Preset Power: 120 / 240</li>
<li>Connection: USB 3.0, backward compatible to 2.0 </li>
<li>Flash Drive Accommodation: Max (W x H) 42mm X 12mm</li>
<li>Weight: 20.4 lbs / 9.2 kg</li>
<li>Dimensions: LxWxH (mm) 200 x 200 x 130</li>
</ul>

<p>USB200PRO SPECIFICATIONS</p>

<ul>
<li>Host PC requirements:</li>
<li>2.0 Dual Core Processor or better</li>
<li>2GB RAM</li>
<li>Windows XP (SP 2+) or Windows 7 32/64</li>
<li>One USB 3.0 High Speed Port</li>
<li>Windows .NET Installed</li>
<li>Preset Power: 120 / 240</li>
<li>Connection: USB 3.0, backward compatible to 2.0 </li>
<li>Flash Drive Accommodation: Max (W x H) 42mm X 12mm</li>
<li>Weight: 20.4 lbs / 9.2 kg</li>
<li>Dimensions: LxWxH (mm) 200 x 200 x 130</li>
</ul>

<p>Product specifiations can change without notice.  Contact Nexcopy for details.  Nexcopy is not responsible for errors posted as either text or images on reseller websites.</p>