Secure Digital Flash Memory Duplicator - SD400PC

Nexcopy introduces the all new Secure Digital Duplicator or the SD Duplicator, the SD400PC. With advanced copy features, small foot print and simple operation, the SD400PC is an economical solution for data loading and data distribution to SD flash memory.

Easy as a photocopier. With advanced software features and friendly user interface,  copy 40 blank SD cards, simply and automatically.   No “copy-n-paste.”  No single card data loading.  No hassles.  The SD400PC is a high performance, PC based flash memory duplicator.

ADVANCED FEATURES

- Data Collection to extract content off cards
   [Ideal for Schools and Universities] 
- Select Bit-for-Bit binary copy from a Master device
   [Ideal for Linux distro’s or bootable flash memory]
- Toggle OFF Read Only Volumes 
   [Ideal for duplication of Partitioned cards]
- Powerful API for custom integration*
- Toggle ON/OFF Windows drive letter mapping
- Unique Data Steaming to SD flash memory*
- Selectable bit for bit Verification feature
- Modular design with flexible configurations

KEY FEATURES

- Copy 40 SD cards quickly and automatically
- Supports SDHC formats & miniSD/microSD sizes
- Job Wizard to run multiple tasks
- Erase, Format, Volume name flash memory cards
- Copy Add to update existing files on flash memory
- Software does not use Windows drive letters
- Modular design, easily expand to 60 ports
- Use as 40 port duplicator, or two 20 port duplicators
- Embedded Check Sum verification
- Clearly marked SD ports on bezel to ID specific devices
- Retro style design with heavy duty case for 24/7 operation 

PC System Requirements:

2.0 Dual Core Processor or better
2GB RAM Ideal
Windows XP (SP 2)
3 USB 2.0 High Speed Ports
Windows .NET Installed

SD400PC Specifications:

Power: Auto detects 120 / 240
Supports SDHC formats
Operating Temp: 10 - 120°F
Weight: 13.6 lbs / 6.1 kg
Dimensions: LxWxH (mm) 200 x 200 x 270